Init680x0() called
Building CPU table for configuration: 68040/68040 prefetch
1867 CPU functions
Building CPU, 46210 opcodes (4 1 0)
CPU=68040, MMU=68040, FPU=68040 ($40), JIT=0.
68040 MMU: enabled=0 page8k=0
scsi disk reset
Changes for:
scsi disk reset
- reset
Memory init: Memory size: 64MB
Mapping Bank0 at $04000000: 16MB
Mapping Bank1 at $05000000: 16MB
Mapping Bank2 at $06000000: 16MB
Mapping Bank3 at $07000000: 16MB
Mapping mirrors of main memory for memory write functions:
Function0 at $10000000
Function1 at $14000000
Function2 at $18000000
Function3 at $1C000000
Mapping Video Memory at $0b000000: 256kB
Mapping mirrors of video memory for memory write functions:
Function0 at $0C000000
Function1 at $0D000000
Function2 at $0E000000
Function3 at $0F000000
Read ROM 131072
68040 MMU: enabled=0 page8k=0
done.
Memory init: Memory size: 64MB
Mapping Bank0 at $04000000: 16MB
Mapping Bank1 at $05000000: 16MB
Mapping Bank2 at $06000000: 16MB
Mapping Bank3 at $07000000: 16MB
Mapping mirrors of main memory for memory write functions:
Function0 at $10000000
Function1 at $14000000
Function2 at $18000000
Function3 at $1C000000
Mapping Video Memory at $0b000000: 256kB
Mapping mirrors of video memory for memory write functions:
Function0 at $0C000000
Function1 at $0D000000
Function2 at $0E000000
Function3 at $0F000000
Read ROM 131072
68040 MMU: enabled=0 page8k=0
bmap lput at 020c0008 val=0 PC=01000028
68040 MMU: enabled=0 page8k=0
68040 MMU: enabled=1 page8k=1
bmap lput at 020c0004 val=c7000000 PC=0100004c
bmap lget at 020c0004 PC=01000742
bmap lput at 020c0004 val=c7000000 PC=0100074c
bmap lput at 020c001c val=70000000 PC=01000756
bmap lput at 020c0020 val=ffffffff PC=01000764
bmap lput at 020c0024 val=ffffffff PC=01000764
bmap lput at 020c0028 val=ffffffff PC=01000764
bmap lput at 020c002c val=ffffffff PC=01000764
bmap lget at 020c0014 PC=0100076a
bmap lget at 020c0010 PC=01000770
bmap lput at 820c0020 val=0 PC=010007a0
bmap lput at 820c0024 val=0 PC=010007a0
bmap lput at 820c0028 val=0 PC=010007a0
bmap lput at 820c002c val=0 PC=010007a0
bmap lget at 020c0014 PC=010007a6
bmap lget at 020c0010 PC=010007ac
bmap lput at 020c001c val=50000000 PC=010007e6
bmap lput at 020c0020 val=0 PC=010007f4
bmap lput at 020c0024 val=0 PC=010007f4
bmap lput at 020c0028 val=0 PC=010007f4
bmap lput at 020c002c val=0 PC=010007f4
bmap lget at 020c0014 PC=010007fa
bmap lget at 020c0010 PC=01000800
bmap lput at 020c001c val=30000000 PC=0100091c
bmap lput at 020c0018 val=0 PC=01000926
bmap lput at 020c0020 val=0 PC=01000934
bmap lput at 020c0024 val=0 PC=01000934
bmap lput at 020c0028 val=0 PC=01000934
bmap lput at 020c002c val=0 PC=01000934
bmap lget at 020c0014 PC=0100093a
bmap lget at 020c0010 PC=01000940
bmap lput at 020c0018 val=e0040028 PC=01000972
bmap lput at 020c001c val=90000000 PC=0100097c
bmap lput at 020c0020 val=0 PC=0100098a
bmap lput at 020c0024 val=0 PC=0100098a
bmap lput at 020c0028 val=0 PC=0100098a
bmap lput at 020c002c val=0 PC=0100098a
bmap lget at 020c0014 PC=01000990
bmap lget at 020c0010 PC=01000996
bmap lput at 020c0018 val=c8080051 PC=010009cc
bmap lput at 020c001c val=b0000000 PC=010009d6
bmap lput at 020c000c val=80000000 PC=01000062
bmap lput at 020c0038 val=e1000000 PC=0100006c
bmap lput at 020c0000 val=0 PC=0100008e
bmap bget at 020c0008 PC=0100452a
bmap bput at 020c0008 val=80 PC=01004530
bmap bget at 020c0008 PC=01004578
bmap bget at 020c0008 PC=0100452a
bmap bput at 020c0008 val=80 PC=01004530
bmap bget at 020c0008 PC=01004578
bmap bget at 020c0008 PC=0100452a
bmap bput at 020c0008 val=80 PC=01004530
bmap bget at 020c0008 PC=01004578
bmap bget at 020c0008 PC=0100452a
bmap bput at 020c0008 val=80 PC=01004530
bmap bget at 020c0008 PC=01004578
bmap bget at 020c0008 PC=010045ec
bmap bput at 020c0008 val=0 PC=010045f2
bmap lget at 020c0030 PC=0100360a
bmap lput at 020c0030 val=90000000 PC=01003618
bmap lget at 020c0034 PC=01003618
bmap lput at 020c0034 val=0 PC=01003626
bmap lget at 020c0034 PC=01007fea
bmap lget at 020c0034 PC=01007fea
bmap lget at 020c0034 PC=01007fea
68040 MMU: enabled=0 page8k=0
68040 MMU: enabled=1 page8k=1
bmap lget at 020c0030 PC=010014ae
bmap lput at 020c0030 val=90000000 PC=010014bc
bmap lget at 020c0034 PC=010014bc
bmap lput at 020c0034 val=0 PC=010014ca
68040 MMU: enabled=0 page8k=0
68040 MMU: enabled=1 page8k=1
bmap bget at 020c000c PC=0408271e
bmap bput at 020c000c val=a0 PC=04082756
bmap lget at 020c0004 PC=01000696
68040 MMU: enabled=0 page8k=0
68040 MMU: enabled=1 page8k=1
bmap lget at 020c0004 PC=01000742
bmap lput at 020c0004 val=c7000000 PC=0100074c
bmap lput at 020c001c val=70000000 PC=01000756
bmap lput at 020c0020 val=ffffffff PC=01000764
bmap lput at 020c0024 val=ffffffff PC=01000764
bmap lput at 020c0028 val=ffffffff PC=01000764
bmap lput at 020c002c val=ffffffff PC=01000764
bmap lget at 020c0014 PC=0100076a
bmap lget at 020c0010 PC=01000770
bmap lput at 820c0020 val=0 PC=010007a0
bmap lput at 820c0024 val=0 PC=010007a0
bmap lput at 820c0028 val=0 PC=010007a0
bmap lput at 820c002c val=0 PC=010007a0
bmap lget at 020c0014 PC=010007a6
bmap lget at 020c0010 PC=010007ac
bmap lput at 020c001c val=50000000 PC=010007e6
bmap lput at 020c0020 val=0 PC=010007f4
bmap lput at 020c0024 val=0 PC=010007f4
bmap lput at 020c0028 val=0 PC=010007f4
bmap lput at 020c002c val=0 PC=010007f4
bmap lget at 020c0014 PC=010007fa
bmap lget at 020c0010 PC=01000800
bmap lput at 020c001c val=30000000 PC=0100091c
bmap lput at 020c0018 val=0 PC=01000926
bmap lput at 020c0020 val=0 PC=01000934
bmap lput at 020c0024 val=0 PC=01000934
bmap lput at 020c0028 val=0 PC=01000934
bmap lput at 020c002c val=0 PC=01000934
bmap lget at 020c0014 PC=0100093a
bmap lget at 020c0010 PC=01000940
bmap lput at 020c0018 val=e0040028 PC=01000972
bmap lput at 020c001c val=90000000 PC=0100097c
bmap lput at 020c0020 val=0 PC=0100098a
bmap lput at 020c0024 val=0 PC=0100098a
bmap lput at 020c0028 val=0 PC=0100098a
bmap lput at 020c002c val=0 PC=0100098a
bmap lget at 020c0014 PC=01000990
bmap lget at 020c0010 PC=01000996
bmap lput at 020c0018 val=c8080051 PC=010009cc
bmap lput at 020c001c val=b0000000 PC=010009d6
68040 MMU: enabled=0 page8k=0
68040 MMU: enabled=1 page8k=1
bmap lput at 020c0004 val=c7000000 PC=0100073c
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 2 OP=F210-4C00 EA=03FFFC34 PC=05048276 -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF95C PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF868 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF854 PC=0504826C -> 040A0CAA
FPU EXCEPTION 3 OP=F210-7C00 EA=03FFF854 PC=0504826C -> 040A0CAA
bmap lget at 020c0034 PC=0408e59a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408f014
bmap lget at 020c0034 PC=0408e59a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408f014
bmap lget at 020c0034 PC=0408e59a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408f014
bmap lget at 020c0034 PC=0408e59a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408e854
bmap lget at 020c0034 PC=0408e912
bmap lget at 020c0034 PC=0408e97c
bmap lput at 020c0034 val=90000000 PC=0408e98a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408f014
bmap lget at 020c0034 PC=0408e59a
bmap lget at 020c0034 PC=0408ef8c
bmap lget at 020c0034 PC=0408f014
bmap bget at 020c000c PC=0408271e
bmap bput at 020c000c val=a0 PC=04082756
bmap bget at 020c000c PC=0408176a
bmap bput at 020c000c val=a0 PC=04081776
bmap bget at 020c000c PC=0408274a
bmap bput at 020c000c val=80 PC=04082756
