Previous 0.5, compiled on:  Jun 10 2014, 16:05:13
Forcing RTC checksum to 70 1a
Loading SCSI disks:
SCSI Disk0: C:\Documents and Settings\Administrator\Desktop\Openstep 4.2 HD Image With Previous\OS42_2GB.dd
SCSI Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk2: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk3: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk4: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk5: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk6: C:\Documents and Settings\Administrator\Desktop\next
Loading magneto-optical disks:
MO Disk0: C:\Documents and Settings\Administrator\Desktop\next
MO Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCC: Device Reset
Forcing RTC checksum to 70 1a
Loading SCSI disks:
SCSI Disk0: C:\Documents and Settings\Administrator\Desktop\Openstep 4.2 HD Image With Previous\OS42_2GB.dd
SCSI Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk2: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk3: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk4: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk5: C:\Documents and Settings\Administrator\Desktop\next
SCSI Disk6: C:\Documents and Settings\Administrator\Desktop\next
Loading magneto-optical disks:
MO Disk0: C:\Documents and Settings\Administrator\Desktop\next
MO Disk1: C:\Documents and Settings\Administrator\Desktop\next
SCC: Device Reset
Host system has accurate delays. (2)
SID read at $0200c800 PC=$0100006c
SCR2 ROM change at $0200d003 val=80 PC=$01000086
SCR1 read at $0200c000 PC=$010000a2
SCR1 read at $0200c001 PC=$010000a2
SCR1 read at $0200c002 PC=$010000a2
SCR1 read at $0200c003 PC=$010000a2
SCR1 read at $0200c000 PC=$010000c2
SCR1 read at $0200c001 PC=$010000c2
SCR1 read at $0200c002 PC=$010000c2
SCR1 read at $0200c003 PC=$010000c2
SCR1 read at $0200c000 PC=$010000fa
SCR1 read at $0200c001 PC=$010000fa
SCR1 read at $0200c002 PC=$010000fa
SCR1 read at $0200c003 PC=$010000fa
IO write at $02106010 val=06 PC=$01000152
IO write at $02106011 val=24 PC=$01000152
IO write at $02106012 val=68 PC=$01000152
IO write at $02106013 val=10 PC=$01000152
IO write at $02106014 val=00 PC=$01000152
Interrupt mask: 00000000
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
SCR1 read at $0200c000 PC=$010001f2
SCR1 read at $0200c001 PC=$010001f2
SCR1 read at $0200c002 PC=$010001f2
SCR1 read at $0200c003 PC=$010001f2
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[RTC] reading val $94 from addr $00 at PC=$01007844
[RTC] reading val $0F from addr $01 at PC=$01007844
[RTC] reading val $40 from addr $02 at PC=$01007844
[RTC] reading val $00 from addr $03 at PC=$01007844
[RTC] reading val $00 from addr $04 at PC=$01007844
[RTC] reading val $00 from addr $05 at PC=$01007844
[RTC] reading val $0F from addr $06 at PC=$01007844
[RTC] reading val $00 from addr $07 at PC=$01007844
[RTC] reading val $F3 from addr $08 at PC=$01007844
[RTC] reading val $02 from addr $09 at PC=$01007844
[RTC] reading val $FB from addr $0A at PC=$01007844
[RTC] reading val $6D from addr $0B at PC=$01007844
[RTC] reading val $00 from addr $0C at PC=$01007844
[RTC] reading val $00 from addr $0D at PC=$01007844
[RTC] reading val $4B from addr $0E at PC=$01007844
[RTC] reading val $00 from addr $0F at PC=$01007844
[RTC] reading val $00 from addr $10 at PC=$01007844
[RTC] reading val $00 from addr $11 at PC=$01007844
[RTC] reading val $73 from addr $12 at PC=$01007844
[RTC] reading val $64 from addr $13 at PC=$01007844
[RTC] reading val $00 from addr $14 at PC=$01007844
[RTC] reading val $00 from addr $15 at PC=$01007844
[RTC] reading val $00 from addr $16 at PC=$01007844
[RTC] reading val $00 from addr $17 at PC=$01007844
[RTC] reading val $00 from addr $18 at PC=$01007844
[RTC] reading val $00 from addr $19 at PC=$01007844
[RTC] reading val $00 from addr $1A at PC=$01007844
[RTC] reading val $00 from addr $1B at PC=$01007844
[RTC] reading val $00 from addr $1C at PC=$01007844
[RTC] reading val $00 from addr $1D at PC=$01007844
[RTC] reading val $70 from addr $1E at PC=$01007844
[RTC] reading val $1A from addr $1F at PC=$01007844
SCR1 read at $0200c000 PC=$010095ce
SCR1 read at $0200c001 PC=$010095ce
SCR1 read at $0200c002 PC=$010095ce
SCR1 read at $0200c003 PC=$010095ce
[RTC] reading val $94 from addr $00 at PC=$01007844
[RTC] reading val $0F from addr $01 at PC=$01007844
[RTC] reading val $40 from addr $02 at PC=$01007844
[RTC] reading val $00 from addr $03 at PC=$01007844
[RTC] reading val $00 from addr $04 at PC=$01007844
[RTC] reading val $00 from addr $05 at PC=$01007844
[RTC] reading val $0F from addr $06 at PC=$01007844
[RTC] reading val $00 from addr $07 at PC=$01007844
[RTC] reading val $F3 from addr $08 at PC=$01007844
[RTC] reading val $02 from addr $09 at PC=$01007844
[RTC] reading val $FB from addr $0A at PC=$01007844
[RTC] reading val $6D from addr $0B at PC=$01007844
[RTC] reading val $00 from addr $0C at PC=$01007844
[RTC] reading val $00 from addr $0D at PC=$01007844
[RTC] reading val $4B from addr $0E at PC=$01007844
[RTC] reading val $00 from addr $0F at PC=$01007844
[RTC] reading val $00 from addr $10 at PC=$01007844
[RTC] reading val $00 from addr $11 at PC=$01007844
[RTC] reading val $73 from addr $12 at PC=$01007844
[RTC] reading val $64 from addr $13 at PC=$01007844
[RTC] reading val $00 from addr $14 at PC=$01007844
[RTC] reading val $00 from addr $15 at PC=$01007844
[RTC] reading val $00 from addr $16 at PC=$01007844
[KMS] Device 1 disabled (mask: 00000000)
[RTC] reading val $00 from addr $17 at PC=$01007844
[RTC] reading val $00 from addr $18 at PC=$01007844
[RTC] reading val $00 from addr $19 at PC=$01007844
[RTC] reading val $00 from addr $1A at PC=$01007844
[RTC] reading val $00 from addr $1B at PC=$01007844
[RTC] reading val $00 from addr $1C at PC=$01007844
[RTC] reading val $00 from addr $1D at PC=$01007844
[RTC] reading val $70 from addr $1E at PC=$01007844
[RTC] reading val $1A from addr $1F at PC=$01007844
SCR1 read at $0200c002 PC=$0100a262
SCR1 read at $0200c002 PC=$0100a55e
[KMS] Device 1 disabled (mask: 00000000)
IO write at $02110000 val=50 PC=$0100a62c
[RTC] reading val $94 from addr $00 at PC=$01007844
[RTC] reading val $0F from addr $01 at PC=$01007844
[RTC] reading val $40 from addr $02 at PC=$01007844
[RTC] reading val $00 from addr $03 at PC=$01007844
[RTC] reading val $00 from addr $04 at PC=$01007844
[RTC] reading val $00 from addr $05 at PC=$01007844
[RTC] reading val $0F from addr $06 at PC=$01007844
[RTC] reading val $00 from addr $07 at PC=$01007844
[RTC] reading val $F3 from addr $08 at PC=$01007844
[RTC] reading val $02 from addr $09 at PC=$01007844
[RTC] reading val $FB from addr $0A at PC=$01007844
[RTC] reading val $6D from addr $0B at PC=$01007844
[RTC] reading val $00 from addr $0C at PC=$01007844
[RTC] reading val $00 from addr $0D at PC=$01007844
[RTC] reading val $4B from addr $0E at PC=$01007844
[RTC] reading val $00 from addr $0F at PC=$01007844
[RTC] reading val $00 from addr $10 at PC=$01007844
[RTC] reading val $00 from addr $11 at PC=$01007844
[RTC] reading val $73 from addr $12 at PC=$01007844
[RTC] reading val $64 from addr $13 at PC=$01007844
[RTC] reading val $00 from addr $14 at PC=$01007844
[RTC] reading val $00 from addr $15 at PC=$01007844
[RTC] reading val $00 from addr $16 at PC=$01007844
[RTC] reading val $00 from addr $17 at PC=$01007844
[RTC] reading val $00 from addr $18 at PC=$01007844
[RTC] reading val $00 from addr $19 at PC=$01007844
[RTC] reading val $00 from addr $1A at PC=$01007844
[RTC] reading val $00 from addr $1B at PC=$01007844
[RTC] reading val $00 from addr $1C at PC=$01007844
[RTC] reading val $00 from addr $1D at PC=$01007844
[RTC] reading val $70 from addr $1E at PC=$01007844
[RTC] reading val $1A from addr $1F at PC=$01007844
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
SCR1 read at $0200c000 PC=$01000b54
SCR1 read at $0200c001 PC=$01000b54
SCR1 read at $0200c002 PC=$01000b54
SCR1 read at $0200c003 PC=$01000b54
[KMS] Device 1 disabled (mask: 00000000)
SCR1 read at $0200c000 PC=$01000bca
SCR1 read at $0200c001 PC=$01000bca
SCR1 read at $0200c002 PC=$01000bca
SCR1 read at $0200c003 PC=$01000bca
[RTC] reading val $94 from addr $00 at PC=$01007844
[RTC] reading val $0F from addr $01 at PC=$01007844
[RTC] reading val $40 from addr $02 at PC=$01007844
[RTC] reading val $00 from addr $03 at PC=$01007844
[RTC] reading val $00 from addr $04 at PC=$01007844
[RTC] reading val $00 from addr $05 at PC=$01007844
[RTC] reading val $0F from addr $06 at PC=$01007844
[RTC] reading val $00 from addr $07 at PC=$01007844
[RTC] reading val $F3 from addr $08 at PC=$01007844
[RTC] reading val $02 from addr $09 at PC=$01007844
[RTC] reading val $FB from addr $0A at PC=$01007844
[RTC] reading val $6D from addr $0B at PC=$01007844
[RTC] reading val $00 from addr $0C at PC=$01007844
[RTC] reading val $00 from addr $0D at PC=$01007844
[RTC] reading val $4B from addr $0E at PC=$01007844
[RTC] reading val $00 from addr $0F at PC=$01007844
[RTC] reading val $00 from addr $10 at PC=$01007844
[RTC] reading val $00 from addr $11 at PC=$01007844
[RTC] reading val $73 from addr $12 at PC=$01007844
[RTC] reading val $64 from addr $13 at PC=$01007844
[RTC] reading val $00 from addr $14 at PC=$01007844
[RTC] reading val $00 from addr $15 at PC=$01007844
[RTC] reading val $00 from addr $16 at PC=$01007844
[RTC] reading val $00 from addr $17 at PC=$01007844
[RTC] reading val $00 from addr $18 at PC=$01007844
[RTC] reading val $00 from addr $19 at PC=$01007844
[RTC] reading val $00 from addr $1A at PC=$01007844
[RTC] reading val $00 from addr $1B at PC=$01007844
[RTC] reading val $00 from addr $1C at PC=$01007844
[RTC] reading val $00 from addr $1D at PC=$01007844
[RTC] reading val $70 from addr $1E at PC=$01007844
[RTC] reading val $1A from addr $1F at PC=$01007844
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
[KMS] Device 1 disabled (mask: 00000000)
SCR1 read at $0200c000 PC=$010045f8
SCR1 read at $0200c001 PC=$010045f8
SCR1 read at $0200c002 PC=$010045f8
SCR1 read at $0200c003 PC=$010045f8
IO write at $02106010 val=19 PC=$01004642
IO write at $02106011 val=38 PC=$01004642
IO write at $02106012 val=68 PC=$01004642
IO write at $02106013 val=10 PC=$01004642
IO write at $02106014 val=00 PC=$01004642
[KMS] Access keyboard/mouse register
[KMS] Data = EF000000
Keyboard/Mouse: Set address to 0
[KMS] Access keyboard/mouse register
[KMS] Data = 00030000
Writing keyboard 0, register 0
Turn on keyboard LED1
Turn on keyboard LED2
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
SCC A, Reg0 read: ff
SCC A, Reg9 write: ca
SCC: Device Reset
SCC A, Reg4 write: 44
SCC A, Reg11 write: 50
SCC A, Reg14 write: 10
SCC A, Reg12 write: 0a
SCC A, Reg13 write: 00
SCC A, Reg14 write: 11
SCC A, Reg10 write: 00
SCC A, Reg3 write: c1
SCC A, Reg5 write: ea
SCC A, Reg15 write: 00
SCC B, Reg15 read: 00
SCC B, Reg4 write: 44
SCC B, Reg11 write: 50
SCC B, Reg14 write: 10
SCC B, Reg12 write: 0a
SCC B, Reg13 write: 00
SCC B, Reg14 write: 11
SCC B, Reg10 write: 00
SCC B, Reg3 write: c1
SCC B, Reg5 write: ea
SCC B, Reg15 write: 00
SCC A, Reg15 read: 00
SCC A, Reg0 read: ff
SCC A, Data write: 40
SCC A, Reg0 read: 05
SCC A, Data read: 40
SCC B, Reg0 read: ff
SCC B, Reg0 read: ff
SCC B, Data write: 40
SCC B, Reg0 read: 05
SCC B, Data read: 40
IO read at $02114108 PC=$0100338c
IO write at $02114108 val=00 PC=$01003394
[EN] Reset write at $02106006 val=$80 PC=$01007d48
[EN] Transmitter masks write at $02106001 val=$00 PC=$01007d4c
[EN] Receiver masks write at $02106003 val=$00 PC=$01007d50
[EN] Transmitter status write at $02106000 val=$ff PC=$01007d52
[EN] Receiver status write at $02106002 val=$ff PC=$01007d56
[EN] Receiver mode write at $02106005 val=$00 PC=$01007d5a
[EN] MAC byte 0 write at $02106008 val=$00 PC=$01006f44
[EN] MAC byte 1 write at $02106009 val=$00 PC=$01006f44
[EN] MAC byte 2 write at $0210600a val=$0f PC=$01006f44
[EN] MAC byte 3 write at $0210600b val=$00 PC=$01006f44
[EN] MAC byte 4 write at $0210600c val=$f3 PC=$01006f44
[EN] MAC byte 5 write at $0210600d val=$02 PC=$01006f44
[EN] Receiver mode write at $02106005 val=$02 PC=$01008254
Interrupt mask: 08000000
[EN] Reset write at $02106006 val=$00 PC=$01007e0a
Starting Ethernet Transmitter/Receiver
[EN] Transmitter mode write at $02106004 val=$02 PC=$010035fe
[EN] Transmitter mode write at $02106004 val=$00 PC=$0100360a
[EN] Transmitter status read at $02106000 val=$80 PC=$01007f84
[EN] Transmitter status write at $02106000 val=$ff PC=$01007f8c
[EN] Sending packet to 00:00:0F:00:F3:02
[EN] Transmitter status read at $02106000 val=$80 PC=$01008006
[EN] Receiving packet from 00:00:0F:00:F3:02
[EN] Receiving packet: Transfer complete.
[EN] Receiver status read at $02106002 val=$80 PC=$010080e4
[EN] Receiver status write at $02106002 val=$ff PC=$010080fa
[EN] Receiver mode write at $02106005 val=$02 PC=$01008254
[EN] MAC byte 5 write at $0210600d val=$03 PC=$0100372a
[EN] Transmitter status read at $02106000 val=$a0 PC=$01007f84
[EN] Transmitter status write at $02106000 val=$ff PC=$01007f8c
[EN] Sending packet to 00:00:0F:00:F3:02
[EN] Transmitter status read at $02106000 val=$a0 PC=$01008006
[EN] Transmitter status read at $02106000 val=$a0 PC=$01007f84
[EN] Transmitter status write at $02106000 val=$ff PC=$01007f8c
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$a0 PC=$01008006
[EN] Receiving packet from 00:00:0F:00:F3:02
[EN] Receiving packet: Transfer complete.
[EN] Receiver status read at $02106002 val=$80 PC=$010080e4
[EN] Receiver status write at $02106002 val=$ff PC=$010080fa
[EN] Receiver mode write at $02106005 val=$02 PC=$01008254
[EN] Transmitter mode write at $02106004 val=$02 PC=$01003806
[EN] Reset write at $02106006 val=$80 PC=$0100808e
Stopping Ethernet Transmitter/Receiver
[RTC] reading val $00 from addr $30 at PC=$01007844
[RTC] writing val $00 to addr $B2 at PC=$01007756
[RTC] reading val $00 from addr $30 at PC=$01007844
[RTC] writing val $B0 to addr $B1 at PC=$01007756
[RTC] reading val $00 from addr $30 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $52 from addr $20 at PC=$01007844
[RTC] reading val $53 from addr $20 at PC=$01007844
Interrupt mask: 20000000
Interrupt mask: 08000000
Interrupt mask: 00800000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Sound out command:
[KMS] Sound out enable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
Interrupt mask: 08000000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
Interrupt mask: 00800000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Sound out command:
[KMS] Sound out enable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
Interrupt mask: 08000000
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
ESP Command: Illegal command!
Interrupt mask: 00000000
IO write at $02118004 val=09 PC=$0100791a
IO write at $02118004 val=c0 PC=$0100791e
SCC A, Reg9 write: 02
SCC A, Reg11 write: 50
SCC A, Reg48 write: 10
SCC A, Reg4 write: 44
SCC A, Reg3 write: c0
SCC A, Reg5 write: 60
SCC A, Reg14 write: 00
IO write at $02118004 val=0a PC=$01007a0a
SCC A, Reg12 write: 0a
SCC A, Reg13 write: 00
SCC A, Reg14 write: 02
SCC A, Reg14 write: 03
SCC A, Reg3 write: c1
SCC A, Reg5 write: ea
SCC B, Reg9 write: 02
SCC B, Reg11 write: 50
SCC B, Reg48 write: 10
SCC B, Reg4 write: 44
SCC B, Reg3 write: c0
SCC B, Reg5 write: 60
SCC B, Reg14 write: 00
IO write at $02118004 val=0a PC=$01007a0a
SCC B, Reg12 write: 0a
SCC B, Reg13 write: 00
SCC B, Reg14 write: 02
SCC B, Reg14 write: 03
SCC B, Reg3 write: c1
SCC B, Reg5 write: ea
[RTC] reading val $00 from addr $30 at PC=$01007844
[RTC] writing val $00 to addr $B2 at PC=$01007756
IO write at $02110000 val=50 PC=$0100a62c
[EN] Reset write at $02106006 val=$80 PC=$010014a6
[EN] Transmitter mode write at $02106004 val=$02 PC=$010014ae
IO read at $02114108 PC=$0100a66a
IO write at $02114108 val=00 PC=$0100a672
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC1C8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($07FFC198).
SCR1 read at $0200c002 PC=$043808de
IO read at $02114108 PC=$04387032
IO write at $02114108 val=00 PC=$04387032
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($043B8FF8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($043B8FC8).
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($043B8FC8).
SCR1 read at $0200c000 PC=$04094b60
SCR1 read at $0200c001 PC=$04094b60
SCR1 read at $0200c002 PC=$04094b60
SCR1 read at $0200c003 PC=$04094b60
Interrupt mask: 00000000
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
IO write at $02110000 val=50 PC=$0408a34e
[KMS] Access keyboard/mouse register
[KMS] Data = EF000000
Keyboard/Mouse: Set address to 0
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
Interrupt mask: 00000004
Interrupt mask: 80000004
Interrupt mask: 8000000c
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[RTC] reading val $00 from addr $30 at PC=$04091c3c
[RTC] writing val $94 to addr $80 at PC=$04091afe
[RTC] writing val $0F to addr $81 at PC=$04091afe
[RTC] writing val $40 to addr $82 at PC=$04091afe
[RTC] writing val $00 to addr $83 at PC=$04091afe
[RTC] writing val $00 to addr $84 at PC=$04091afe
[RTC] writing val $00 to addr $85 at PC=$04091afe
[RTC] writing val $0F to addr $86 at PC=$04091afe
[RTC] writing val $00 to addr $87 at PC=$04091afe
[RTC] writing val $F3 to addr $88 at PC=$04091afe
[RTC] writing val $02 to addr $89 at PC=$04091afe
[RTC] writing val $FB to addr $8A at PC=$04091afe
[RTC] writing val $6D to addr $8B at PC=$04091afe
[RTC] writing val $00 to addr $8C at PC=$04091afe
[RTC] writing val $00 to addr $8D at PC=$04091afe
[RTC] writing val $4B to addr $8E at PC=$04091afe
[RTC] writing val $00 to addr $8F at PC=$04091afe
[RTC] writing val $00 to addr $90 at PC=$04091afe
[RTC] writing val $00 to addr $91 at PC=$04091afe
[RTC] writing val $73 to addr $92 at PC=$04091afe
[RTC] writing val $64 to addr $93 at PC=$04091afe
[RTC] writing val $00 to addr $94 at PC=$04091afe
[RTC] writing val $00 to addr $95 at PC=$04091afe
[RTC] writing val $00 to addr $96 at PC=$04091afe
[RTC] writing val $00 to addr $97 at PC=$04091afe
[RTC] writing val $00 to addr $98 at PC=$04091afe
[RTC] writing val $00 to addr $99 at PC=$04091afe
[RTC] writing val $00 to addr $9A at PC=$04091afe
[RTC] writing val $00 to addr $9B at PC=$04091afe
[RTC] writing val $00 to addr $9C at PC=$04091afe
[RTC] writing val $00 to addr $9D at PC=$04091afe
[RTC] writing val $70 to addr $9E at PC=$04091afe
[RTC] writing val $1A to addr $9F at PC=$04091afe
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[RTC] reading val $00 from addr $30 at PC=$04091c3c
[RTC] reading val $57 from addr $20 at PC=$04091dac
[RTC] reading val $40 from addr $21 at PC=$04091dac
[RTC] reading val $23 from addr $22 at PC=$04091dac
[RTC] reading val $01 from addr $23 at PC=$04091dac
[RTC] reading val $12 from addr $24 at PC=$04091dac
[RTC] reading val $10 from addr $25 at PC=$04091dac
[RTC] reading val $14 from addr $26 at PC=$04091dac
[RTC] reading val $00 from addr $27 at PC=$04091dac
[RTC] reading val $57 from addr $20 at PC=$04091c3c
Interrupt mask: a000000c
Interrupt mask: a001800f
IO write at $02118004 val=0a PC=$0408d8fa
SCC A, Reg5 write: 00
SCC B, Reg5 write: 00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406c5ca
IO read at $02114108 PC=$0406c5ca
IO write at $02114108 val=40 PC=$0406d09c
IO read at $02114100 PC=$04001880
IO read at $02114101 PC=$04001880
IO read at $02114102 PC=$04001880
IO read at $02114105 PC=$04001880
IO read at $02114107 PC=$04001880
IO write at $02114102 val=04 PC=$0406c6c8
IO read at $02114102 PC=$0406c6c8
IO write at $02114102 val=04 PC=$0406c6dc
IO read at $02114102 PC=$0406c6dc
IO write at $02114102 val=05 PC=$0406c6dc
IO read at $02114102 PC=$0406c6dc
IO write at $02114102 val=06 PC=$0406c6dc
IO read at $02114102 PC=$0406c6dc
IO write at $02114102 val=07 PC=$0406c6dc
IO read at $02114102 PC=$0406c6dc
IO write at $02114102 val=00 PC=$0406cebe
IO write at $02114102 val=04 PC=$0406cece
IO write at $02114104 val=00 PC=$0406ced2
IO write at $02114107 val=00 PC=$0406ced6
IO write at $02114108 val=40 PC=$0406cee2
IO write at $02114108 val=00 PC=$0406d0bc
ESP FIFO read: FIFO is empty!
IO write at $0211400b val=0f PC=$0407acc8
IO write at $0211400b val=00 PC=$0407ace4
Interrupt mask: a401800f
Interrupt mask: a401900f
IO write at $02114108 val=00 PC=$0406d0bc
Interrupt mask: a401900f
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C5998).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 8 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C5998).
IO write at $02114108 val=00 PC=$0406d0bc
[SCSI] Mode Sense: page = 00, page_control = 0, block descriptor enabled
[SCSI] Mode Sense: Block descriptor data: disk is read/write, size = 3931200 blocks, blocksize = 512 byte
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 6 residual bytes in DMA buffer.
[DMA] Channel SCSI: Start memory address is not 16 byte aligned ($040C59C8).
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[EN] MAC byte 0 write at $02106008 val=$00 PC=$04092e0a
[EN] MAC byte 1 write at $02106009 val=$00 PC=$04092e0a
[EN] MAC byte 2 write at $0210600a val=$0f PC=$04092e0a
[EN] MAC byte 3 write at $0210600b val=$00 PC=$04092e0a
[EN] MAC byte 4 write at $0210600c val=$f3 PC=$04092e0a
[EN] MAC byte 5 write at $0210600d val=$02 PC=$04092e0a
[EN] Reset write at $02106006 val=$80 PC=$0408dcf6
Interrupt mask: b401900f
Interrupt mask: b401940f
Interrupt mask: bc01940f
[DSP] write val 0 PC=40818a8 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val -2147483648 PC=4082638 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] read val -2147483648 PC=4082644 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 75
[DSP] write val 50331647 PC=4082672 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] write val 16777215 PC=408268c C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
IO read at $0200f003 PC=$0407499c
IO read at $0200f002 PC=$040749e2
IO write at $0200f002 val=00 PC=$040749ee
Interrupt mask: bd01940f
[KMS] Sound in command
[KMS] Sound in disable.
[KMS] Sound out command:
[KMS] Sound out disable.
[KMS] Sound out normal sample.
[KMS] Sound out sample by repetition.
[KMS] Access volume control logic
[KMS] Data = 000000FF
Interrupt mask: bd01950f
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[RTC] writing val $30 to addr $B1 at PC=$040919ba
[RTC] writing val $08 to addr $A0 at PC=$04091afe
setting 0 to 8
Offset is 1413171660
[RTC] writing val $18 to addr $A1 at PC=$04091afe
setting 1 to 12
Offset is 1413171660
[RTC] writing val $08 to addr $A2 at PC=$04091afe
setting 2 to 8
Offset is 1413171660
[RTC] writing val $01 to addr $A3 at PC=$04091afe
[RTC] writing val $16 to addr $A4 at PC=$04091afe
setting 3 to 10
Offset is 1413171660
[RTC] writing val $04 to addr $A5 at PC=$04091afe
setting 4 to 4
Offset is 1413171660
[RTC] writing val $A9 to addr $A6 at PC=$04091afe
setting 5 to 6d
Offset is 173283771
[RTC] writing val $00 to addr $A7 at PC=$04091afe
[RTC] writing val $B0 to addr $B1 at PC=$040919ba
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 16 residual bytes in DMA buffer.
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 16 residual bytes in DMA buffer.
[DMA] Channel SCSI: 16 residual bytes in DMA buffer.
IO write at $02114108 val=00 PC=$0406d0bc
[DMA] Channel SCSI: 16 residual bytes in DMA buffer.
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[EN] Reset write at $02106006 val=$80 PC=$0408df20
[EN] Transmitter mode write at $02106004 val=$00 PC=$0408df76
[EN] Transmitter status write at $02106000 val=$ff PC=$0408df78
[EN] Transmitter masks write at $02106001 val=$04 PC=$0408df8e
[EN] Receiver status write at $02106002 val=$ff PC=$0400177a
[EN] Receiver masks write at $02106003 val=$00 PC=$0400177a
[EN] Receiver mode write at $02106005 val=$00 PC=$0400177a
[EN] Reset write at $02106006 val=$00 PC=$0408dfe2
Starting Ethernet Transmitter/Receiver
[EN] Transmitter mode write at $02106004 val=$02 PC=$0408dff2
[EN] Receiver mode write at $02106005 val=$01 PC=$0408e000
[EN] Receiver mode write at $02106005 val=$02 PC=$0408f290
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
[EN] Receiver mode write at $02106005 val=$03 PC=$0408ef1a
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
[EN] Receiver mode write at $02106005 val=$02 PC=$0408ef68
[EN] Transmitter mode read at $02106004 val=$02 PC=$0408e98c
[EN] Transmitter mode write at $02106004 val=$00 PC=$0408e998
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$80 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
[EN] Receiving packet from 00:00:0F:00:F3:02
[EN] Receiving packet: Transfer complete.
[EN] Sending packet to FF:FF:FF:FF:FF:FF
[EN] Transmitter status read at $02106000 val=$a0 PC=$0408ede0
[EN] Transmitter status read at $02106000 val=$a0 PC=$0408ee1c
[EN] Transmitter status write at $02106000 val=$ff PC=$0408ee24
[EN] Receiving packet from 00:00:0F:00:F3:02
[EN] Receiving packet: Transfer complete.
Key pressed: left ctrl
Keycode: $00, Modifiers: $00
Key pressed: c
Keycode: $33, Modifiers: $01
IO write at $02114108 val=00 PC=$0406d0bc
Key released: c
Keycode: $33, Modkeys: $01
Key released: left ctrl
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO read at $0200f002 PC=$0407306a
IO write at $0200f002 val=00 PC=$04073076
IO read at $0200f002 PC=$04073076
IO write at $0200f002 val=02 PC=$04073082
IO read at $0200f001 PC=$04073082
IO write at $0200f001 val=80 PC=$0407308e
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO read at $0200f002 PC=$040724ec
IO write at $0200f003 val=ff PC=$04072504
IO read at $0200f000 PC=$0407250e
IO write at $0200f004 val=ff PC=$04072532
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f002 PC=$040724ec
IO write at $0200f003 val=04 PC=$04072504
IO read at $0200f000 PC=$0407250e
IO write at $0200f004 val=00 PC=$04072532
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f000 PC=$04072702
IO read at $0200f000 PC=$0407270a
IO read at $0200f000 PC=$04072712
IO read at $0200f001 PC=$04073150
IO write at $0200f001 val=00 PC=$0407315c
IO read at $0200f002 PC=$0407315c
IO write at $0200f002 val=00 PC=$04073168
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
Interrupt mask: bd01952f
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02110000 val=50 PC=$0408a34e
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 02000000
[KMS] Access volume control logic
[KMS] Data = 06000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 04000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[KMS] Access volume control logic
[KMS] Data = 01000000
[KMS] Access volume control logic
[KMS] Data = 00000000
[DSP] write val 16777215 PC=40818a8 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
[DSP] read val 16777215 PC=40817a2 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 75
[DSP] write val 2147483647 PC=40817c0 C:/MinGW/msys/1.0/home/Administrator/branch_mmu/src/ioMemTabNEXT.c at 81
Interrupt mask: bd01d52f
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Interrupt mask: bd01d52f
Interrupt mask: bd81d52f
Interrupt mask: bdc1d52f
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: return
Keycode: $2a, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: return
Keycode: $2a, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: return
Keycode: $2a, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
Key released: return
Keycode: $2a, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right super
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right super
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right super
Keycode: $00, Modifiers: $00
Key pressed: right super
Keycode: $00, Modifiers: $00
Key pressed: right super
Keycode: $00, Modifiers: $00
Key released: right super
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
[KMS] Access keyboard/mouse register
[KMS] Data = 00000000
Writing keyboard 0, register 0
Turn off keyboard LED1
Turn off keyboard LED2
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02110000 val=50 PC=$0408a34e
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[RTC] writing val $94 to addr $80 at PC=$04091afe
[RTC] writing val $0F to addr $81 at PC=$04091afe
[RTC] writing val $40 to addr $82 at PC=$04091afe
[RTC] writing val $00 to addr $83 at PC=$04091afe
[RTC] writing val $00 to addr $84 at PC=$04091afe
[RTC] writing val $00 to addr $85 at PC=$04091afe
[RTC] writing val $0F to addr $86 at PC=$04091afe
[RTC] writing val $00 to addr $87 at PC=$04091afe
[RTC] writing val $F3 to addr $88 at PC=$04091afe
[RTC] writing val $02 to addr $89 at PC=$04091afe
[RTC] writing val $FB to addr $8A at PC=$04091afe
[RTC] writing val $6D to addr $8B at PC=$04091afe
[RTC] writing val $00 to addr $8C at PC=$04091afe
[RTC] writing val $00 to addr $8D at PC=$04091afe
[RTC] writing val $4B to addr $8E at PC=$04091afe
[RTC] writing val $00 to addr $8F at PC=$04091afe
[RTC] writing val $00 to addr $90 at PC=$04091afe
[RTC] writing val $00 to addr $91 at PC=$04091afe
[RTC] writing val $73 to addr $92 at PC=$04091afe
[RTC] writing val $64 to addr $93 at PC=$04091afe
[RTC] writing val $00 to addr $94 at PC=$04091afe
[RTC] writing val $00 to addr $95 at PC=$04091afe
[RTC] writing val $00 to addr $96 at PC=$04091afe
[RTC] writing val $00 to addr $97 at PC=$04091afe
[RTC] writing val $00 to addr $98 at PC=$04091afe
[RTC] writing val $00 to addr $99 at PC=$04091afe
[RTC] writing val $00 to addr $9A at PC=$04091afe
[RTC] writing val $00 to addr $9B at PC=$04091afe
[RTC] writing val $00 to addr $9C at PC=$04091afe
[RTC] writing val $00 to addr $9D at PC=$04091afe
[RTC] writing val $70 to addr $9E at PC=$04091afe
[RTC] writing val $1A to addr $9F at PC=$04091afe
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02110000 val=50 PC=$0408a34e
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02110000 val=50 PC=$0408a34e
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
[RTC] writing val $94 to addr $80 at PC=$04091afe
[RTC] writing val $0F to addr $81 at PC=$04091afe
[RTC] writing val $40 to addr $82 at PC=$04091afe
[RTC] writing val $00 to addr $83 at PC=$04091afe
[RTC] writing val $00 to addr $84 at PC=$04091afe
[RTC] writing val $00 to addr $85 at PC=$04091afe
[RTC] writing val $0F to addr $86 at PC=$04091afe
[RTC] writing val $00 to addr $87 at PC=$04091afe
[RTC] writing val $F3 to addr $88 at PC=$04091afe
[RTC] writing val $02 to addr $89 at PC=$04091afe
[RTC] writing val $FB to addr $8A at PC=$04091afe
[RTC] writing val $6D to addr $8B at PC=$04091afe
[RTC] writing val $00 to addr $8C at PC=$04091afe
[RTC] writing val $00 to addr $8D at PC=$04091afe
[RTC] writing val $4B to addr $8E at PC=$04091afe
[RTC] writing val $00 to addr $8F at PC=$04091afe
[RTC] writing val $00 to addr $90 at PC=$04091afe
[RTC] writing val $00 to addr $91 at PC=$04091afe
[RTC] writing val $73 to addr $92 at PC=$04091afe
[RTC] writing val $64 to addr $93 at PC=$04091afe
[RTC] writing val $00 to addr $94 at PC=$04091afe
[RTC] writing val $00 to addr $95 at PC=$04091afe
[RTC] writing val $00 to addr $96 at PC=$04091afe
[RTC] writing val $00 to addr $97 at PC=$04091afe
[RTC] writing val $00 to addr $98 at PC=$04091afe
[RTC] writing val $00 to addr $99 at PC=$04091afe
[RTC] writing val $00 to addr $9A at PC=$04091afe
[RTC] writing val $00 to addr $9B at PC=$04091afe
[RTC] writing val $00 to addr $9C at PC=$04091afe
[RTC] writing val $00 to addr $9D at PC=$04091afe
[RTC] writing val $70 to addr $9E at PC=$04091afe
[RTC] writing val $1A to addr $9F at PC=$04091afe
[RTC] reading val $94 from addr $00 at PC=$04091dac
[RTC] reading val $0F from addr $01 at PC=$04091dac
[RTC] reading val $40 from addr $02 at PC=$04091dac
[RTC] reading val $00 from addr $03 at PC=$04091dac
[RTC] reading val $00 from addr $04 at PC=$04091dac
[RTC] reading val $00 from addr $05 at PC=$04091dac
[RTC] reading val $0F from addr $06 at PC=$04091dac
[RTC] reading val $00 from addr $07 at PC=$04091dac
[RTC] reading val $F3 from addr $08 at PC=$04091dac
[RTC] reading val $02 from addr $09 at PC=$04091dac
[RTC] reading val $FB from addr $0A at PC=$04091dac
[RTC] reading val $6D from addr $0B at PC=$04091dac
[RTC] reading val $00 from addr $0C at PC=$04091dac
[RTC] reading val $00 from addr $0D at PC=$04091dac
[RTC] reading val $4B from addr $0E at PC=$04091dac
[RTC] reading val $00 from addr $0F at PC=$04091dac
[RTC] reading val $00 from addr $10 at PC=$04091dac
[RTC] reading val $00 from addr $11 at PC=$04091dac
[RTC] reading val $73 from addr $12 at PC=$04091dac
[RTC] reading val $64 from addr $13 at PC=$04091dac
[RTC] reading val $00 from addr $14 at PC=$04091dac
[RTC] reading val $00 from addr $15 at PC=$04091dac
[RTC] reading val $00 from addr $16 at PC=$04091dac
[RTC] reading val $00 from addr $17 at PC=$04091dac
[RTC] reading val $00 from addr $18 at PC=$04091dac
[RTC] reading val $00 from addr $19 at PC=$04091dac
[RTC] reading val $00 from addr $1A at PC=$04091dac
[RTC] reading val $00 from addr $1B at PC=$04091dac
[RTC] reading val $00 from addr $1C at PC=$04091dac
[RTC] reading val $00 from addr $1D at PC=$04091dac
[RTC] reading val $70 from addr $1E at PC=$04091dac
[RTC] reading val $1A from addr $1F at PC=$04091dac
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
Key pressed: m
Short :2
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: m
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: right alt
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: m
Short :2
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: m
IO write at $02114108 val=00 PC=$0406d0bc
Key released: right alt
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: m
Short :2
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: right alt
Keycode: $00, Modkeys: $00
Key released: m
Keycode: $36, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
Key released: right alt
Keycode: $00, Modkeys: $00
Key pressed: left ctrl
Keycode: $00, Modifiers: $00
Key released: left ctrl
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: m
Short :2
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: m
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: right alt
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key pressed: right alt
Keycode: $00, Modifiers: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
Key released: right alt
Keycode: $00, Modkeys: $00
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
IO write at $02114108 val=00 PC=$0406d0bc
